{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["page 1","Drop Downs","Gas Composition Tab"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"page 1","index":0,"n_rows":49,"n_cols":17,"rows_kept":49,"cut":false,"hidden":false,"merged":[[48,0,48,20],[45,12,45,14],[45,15,45,18],[45,19,45,20],[8,0,8,20],[18,0,18,20],[34,0,34,20],[39,4,39,11],[33,9,33,11],[33,12,33,15],[33,16,33,20],[30,4,30,8],[30,9,30,11],[30,12,30,15],[30,0,33,2],[44,12,44,20],[27,4,27,11],[27,12,27,20],[9,4,9,8],[9,9,9,11],[9,12,9,15],[9,16,9,20],[39,12,39,15],[39,16,39,20],[44,4,44,11],[40,4,40,11],[40,12,40,20],[42,12,42,15],[42,16,42,20],[41,4,41,7],[41,8,41,9],[41,10,41,11],[41,12,41,14],[41,15,41,18],[41,19,41,20],[42,10,42,11],[6,4,6,11],[7,9,7,11],[7,4,7,8],[4,0,7,2],[11,13,11,16],[11,17,11,19],[12,13,12,16],[12,17,12,19],[9,0,17,2],[4,4,4,11],[4,12,4,20],[5,4,5,11],[5,12,5,20],[6,12,6,20],[7,12,7,15],[7,16,7,20],[13,13,13,16],[13,17,13,19],[14,13,14,16],[17,16,17,20],[16,4,16,8],[15,4,15,9],[15,10,15,11],[21,4,21,8],[31,4,31,8],[22,4,22,11],[13,7,13,9],[14,4,14,6],[14,7,14,9],[16,16,16,20],[22,12,22,15],[20,4,20,8],[21,9,21,11],[21,12,21,15],[21,16,21,20],[20,12,20,14],[20,15,20,18],[28,12,28,20],[25,4,25,11],[23,4,23,11],[23,12,23,20],[20,10,20,11],[20,19,20,20],[17,12,17,15],[26,12,26,15],[26,16,26,20],[24,4,24,8],[38,16,38,20],[38,4,38,8],[38,9,38,11],[16,9,16,11],[16,12,16,15],[12,4,12,8],[14,17,14,19],[17,4,17,8],[17,9,17,11],[15,12,15,15],[15,16,15,20],[13,4,13,6],[31,16,31,20],[35,4,35,8],[35,9,35,11],[22,16,22,20],[19,4,19,8],[19,10,19,11],[19,12,19,14],[19,15,19,18],[19,19,19,20],[37,16,37,20],[26,4,26,8],[26,9,26,11],[24,9,24,11],[24,12,24,15],[24,16,24,20],[28,4,28,11],[30,16,30,20],[32,4,32,11],[31,9,31,11],[31,12,31,15],[37,4,37,8],[37,9,37,11],[37,12,37,15],[35,12,35,15],[35,16,35,20],[25,12,25,20],[36,4,36,11],[36,12,36,20],[0,12,3,20],[3,0,3,11],[19,0,28,2],[47,4,47,11],[47,12,47,20],[29,0,29,20],[33,4,33,8],[43,10,43,11],[42,4,42,9],[43,4,43,9],[43,12,43,15],[43,16,43,20],[45,4,45,6],[45,7,45,9],[45,10,45,11],[46,12,46,20],[46,4,46,11],[32,12,32,20],[35,0,47,2],[38,12,38,15],[10,4,10,8],[11,4,11,8],[10,13,10,16],[10,17,10,19]]}
[null,null,null,null,null,null,null,null,null,null,null,null,"GE General Gas/Расходомер газа\nApplication Data Sheet/Опросный лист\nHighlighed Row = Mandatory Field\nВыделеные строки=Обязательны к заполнению"]
[]
[]
["173021, Великий Новгород, ул. Нехинская 61                                                                                тел.: +7 (8162) 94-68-88      факс:+7 (8162) 94-67-75     E.mail:  office@dscontrols.ru"]
["GENERAL/Общие",null,null,1,"Company Name /Компания"]
[null,null,null,2,"Name/Контактное лицо"]
[null,null,null,3,"Address/Адрес"]
[null,null,null,4,"Phone/Тел.",null,null,null,null,"Email"]
[]
["PROCESS CONDITIONS/ Условия процесса",null,null,5,"Tag Number/\nНомер позиции",null,null,null,null,"Gas Composition/\nСостав газа"]
[null,null,null,6,"Flow @ Standard Min.\nРасход@ Мин.",null,null,null,null,"Oper./\nНорм.","Max./\nМакс","Units/\nЕд."]
[null,null,null,7,"Temp. @ Flowrate Min. Температура @ Мин.",null,null,null,null,"Oper./\nНорм.","Max./\nМакс","Units/\nЕд."]
[null,null,null,8,"Press @ Flowrate Min./\nДавление @ Мин.",null,null,null,null,"Oper./\nНорм.","Max./\nМакс","Units/\nЕд."]
[null,null,null,9,"Visc @ Min/ \nВязкость Мин",null,null,"Oper. Viscosity/\nНорм",null,null,"Max./\nМакс","Units/\nЕд."]
[null,null,null,10,"Min MW/ \nМолек. вес \nмин.",null,null,"Oper. MW/ Норм.",null,null,"Max./\nМакс","Units/\nЕд."]
[null,null,null,11,"Corrosive / Abrasive Property./\nАнтикоррозионая защита",null,null,null,null,null,"Build Up/\nОтложения"]
[null,null,null,12,"%Suspended Solids/\nТвердые включения %",null,null,null,null,"% Liquid Droplets/\nНаличие жидкости %"]
[null,null,null,13,"Design Max Press. /\nРасчетное давление",null,null,null,null,"Design Max.Temp./ \nРасчетная темп-ра"]
[]
["TRANSDUCER/\nFLOWCELL\nINSTALLATION/ Установка \nдатчика и измерительного участка",null,null,14,"Pipe Material/\nМатериал труб-да",null,null,null,null,"Pipe Size/\nРазмер \nтруб-да","Wall/Schd. /\nТолщина"]
[null,null,null,15,"Flange Rating/\nРейтинг фланца",null,null,null,null,"Lining/\nФутеровка","Pipe Spec/\nСтандарт \nтрубопровода"]
[null,null,null,16,"Upstream Straight Run\nНаличиие прямолинейного\nучастка до установки\nрасходомера",null,null,null,null,"Downstream /\nпосле установки\n расходомера",null,null,"(Pipe Diameters)/\n(Количество диаметров)",null,null,null,"(Pipe Diameters)/\n(Количество диаметров)"]
[null,null,null,17,"Measurement Location /Место установки",null,null,null,null,null,null,null,null,null,null,null,"(Specify Other)/Другое"]
[null,null,null,18,"Wetted / Clamp-On /\nВрезной/Накладной"]
[null,null,null,19,"Flowcell Required/\nТребуется измерительный \nучасток\n",null,null,null,null,"Isolation Valve (x'ducer)/\nОтсечной клапан\n (для датчика)"]
[null,null,null,20,"Transmitter Housing Requirement \nТребование к пылевлагозащите \nэлектронного блока"]
[null,null,null,21,"Transducer Haz. Area/\nТребование к \nвзрывозащите датчика",null,null,null,null,"Transmitter Haz Area /Требование к \nвзрывозащите\n электронного блока"]
[null,null,null,22,"Ambient Conditions (Corrosive gas, temp, hum)/\nУсловия окружающей среды (коррозионый газ, температура окружающего воздуха, влажность)\n"]
[null,null,null,23,"Required Cable Length (1000 ft. Max)/\nДлина кабеля (макс. 330 метров)"]
[]
["MEASUREMENT\nPARAMETERS/\nПараметры элетронного блока",null,null,24,"Analog Outputs\nАналоговые выходы",null,null,null,null,"Digital/Цифровой "]
[null,null,null,25,"Inputs (P and T)/\nВходы (P и Т)",null,null,null,null,"Alarms / Сигнальное реле"]
[null,null,null,26,"Power Available/ Напряжение питания"]
[null,null,null,27,"Desired Accuracy/\nТребование по\n погрешности",null,null,null,null,"Desired Repeatability/ \nТребования\n по повторяемости"]
[]
["FLOWCELL /Требования к измерительному участку ",null,null,28,"Flowcell Required \nНаличие измерительного участка",null,null,null,null,"Pipe Spec /Спецификация\n треубопровода"]
[null,null,null,29,"NDE Required (LPI, Hydro, X-ray are standard)/\nТребования по НК (Гидротест, Рентген, \nКапиллярная дефектоскопия- стандарт)"]
[null,null,null,30,"Material: Carbon Steel \nМатериал: Углеродистая сталь",null,null,null,null,"Stainless Steel \nНержавеющая сталь"]
[null,null,null,31,"5Cr-1/2Mo / \nХромомолибденовая \nсталь",null,null,null,null,"9Cr-1/2Mo\nХромомолибденовая \nсталь"]
[null,null,null,32,"Other Material :Specify Pipe and Flange /\nДругой материал: Укажите спецификацию \nтрубопровода и фланца",null,null,null,null,null,null,null,"Pipe:/Трубопровод",null,null,null,"Flange:/Фланец"]
[null,null,null,34,"Indicate Flowcell Flanged or Weld Prep Ends /\nУказать способ присоединение к трубопроводу- фланцевый или под приварку",null,null,null,null,null,null,null,"Other"]
[null,null,null,33,"Rating/Рейтинг",null,null,null,"Flange Type/\nТип фланца",null,"Pipe>24\"/\nТруба >24\""]
[null,null,null,35,"Addl Port Pressure - Size/Class\nТребование к присоединению датчика  давления - размер/класс",null,null,null,null,null,"Type /Тип"]
[null,null,null,36,"Addl Port Temp - Size/Class /\nТребование к присоединению датчика  \nтемпературы - размер/класс",null,null,null,null,null,"Type /Тип"]
[null,null,null,37,"Pipe Specification/ Спецификация трубопровода"]
[null,null,null,38,"Design P\nРасчетное давление",null,null,"Design Temp\nРасчетная \nТемпература",null,null,"Corro. Allow. \nПрипуск на коррозию"]
[null,null,null,39,"Paint Sytem /Требование по покраске"]
[null,null,null,40,"Interior Coating /Внутренне покрытие"]
["NOTES: Specify any applicable regulatory information (NSPS Ja, HRVOC, AQMD, Consent Decree)\nТребования по калибровке, хранения данных, наличие сумматора.\nSpecify any clearance issues (Submit Isometric if available)\nДополнение: Укажите дополнительные требования регулирующих органов если они есть (NSPS Ja, HRVOC, AQMD, Consent Decree)\nУкажите дополнительные требования (если имеется дополнительная изометрия трубопровода, просьба предоставить)"]

{"sheet":"Drop Downs","index":1,"n_rows":45,"n_cols":8,"rows_kept":45,"cut":false,"hidden":true,"merged":[]}
["Measurement location","Flowcell Required?","Transducer Removal ","Location","Transducer Haz Area","Transmitter Haz Area","Electronics Housing Requirement "]
["Main Header","Yes","Yes","Hazardous","USA/CAN Div1, Cl1 Gr CD","None, NEMA4X & IP66","Weatherproof, Non-incendive NEMA4X & IP66 (Cl1 Div 2)"]
["Pipe Vertical","No (Hot/Cold Tap)","No","Nonhazardous","USA/CAN Div1, Cl1 Gr BCD","USA/CAN Div2, Cl1 ABCD","Explosionproof NEMA7 / 4X"]
["Before Seal Drum",null,null,"Nonhazardous Weatherproof","ATEX II 2 G Ex d IIC T6","USA/CAN Div1, Cl1 BCD"]
["Before Knock-Out Drum",null,null,null,"IECEx II 2 G Ex d IIC T6","ATEX II 2 G Ex d IIB+H2 T6"]
["Flare Lateral Header",null,null,null,"INMETRO","ATEX II 2 G Ex d IIC T6"]
["Pipe Horizontal ",null,null,null,"Other (Specify in Notes)","IECEx Ex d IIB+H2 T6"]
["After Seal Drum",null,null,null,"General Purpose Area","IECEx Ex d IIC T6"]
["After Knock-out drum",null,null,null,null,"INMETRO"]
["Other",null,null,null,null,"Other (Specify in Notes)"]
[]
[]
[]
["Analog Outputs","Digital Outputs","Alarms","Inputs (Pres./Temp)","Power Available","NDE"]
["Two isolated 4 to 20","None","None","Two isolated 4 to 20","100/120 VAC","X-Ray"]
["Six isolated 4 to 20","Four config. Pulse total/freq. outputs","3 hermetically sealed alarms","Six isolated 4 to 20","220/240 VAC","LPI"]
["Ten isolated 4 to 20","Modbus Digital","6 hermetically sealed alarms","2 isolated 4 to 20 and two RDT","12 to 28 VDC","HydroStatic"]
[null,"Modbus digital + 4 config. Pluse total/freq outputs",null,null,null,"Mag Particle "]
[null,"HART",null,null,null,"PMI"]
[null,"HART + 4 config. Pulse total/freq outputs",null,null,null,"Charpy Impact"]
[null,"MODBUS TCP",null,null,null,"Post Weld Heat Treatment"]
[null,"Ethernet card (panaview/OPC)",null,null,null,"NACE"]
[null,"Foundation Fieldbus",null,null,null,"Brinell Hardness"]
[null,"WiFi Board (Modbus/TCP)",null,null,null,"Others"]
[null,"WiFi Board (panaview/OPC)"]
[]
["Carbon Steel","Stainless Steel","5C-1/2M","9C-1/2M","Flange Rating","Flange Type","Flange Type","Flanged/Weld Prep"]
["ASTM A106 GrB/A105 (Valid to 24\" NPS)","ASTM A312 Gr304/A182 GrF304","ASTM A335 GrP5/A182 GrF5","ASTM A335 GrP9/A182 GrF9",150,"Weldneck","ANSI B16.47A","Flanged "]
["ASTM A672GrC70/A105 (Valid > 24\" NPS)","ASTM A312 Gr316/A182 GrF360","Other (Enter Below)","Other (Enter Below)",300,"Slip-on","ANSI B16.47B","Weld-Prep"]
["ASTM A333 Gr6/A350LF2","Other (Enter Below)",null,null,600,"RTJ",null,"Other"]
["Other (Enter Below)",null,null,null,900,"AWWA"]
[null,null,null,null,1500,"Other (Specify in Notes)"]
[null,null,null,null,2500]
["Port Type","Paint System ","Interior Coating ",null,"Other (Specify in Notes)"]
["Thredolet","System A - Bare Metal (Bare Steel, no coating)","Standard Water Soluable Rust Inhibitor "]
["Sockolet","System B -High Temperature Primer (Dry Temp. Resistance: 750oF/399oC)\n(Surface Prep: Surface prep to near white metal SP-10 / Primer Coat: Carbonic 11 Primer, 3-4 mils DFT, Manufacturer's Color Code 0700 (Gray) / Cure per Manufacturer's specifications)","Special (Specify in Notes, Include Coating spec and paint system)",null,"Gas Composition Tab"]
["Nipple","System C - 1 Coat Epoxy Paint, Self Priming (Dry Temp. Resistance: 425oF/218oC)\n(Surface Prep to near white metal SP-10 / Top Coat: Carboline Thermoline 450 Novalak Glass Filled Epoxy / Manufacturer's Color Code : 5742 (Gray), Cure per Manufacturer's specifications / Self Priming, No primer coat needed)","None",null,"Attaching Gas Composition to ADS"]
["Flanged","System D - 2 Coat Silicone Paint (Dry Temp. Resistance: 1000oF/538oC)\n(Surface Prep: Surface prep to near white metal SP-10 / Primer Coat: Carbozinc 11 Primer 3-4 mils DFT / Top Coat: Carboline Thermoline 4700, 2 coat at 1.5 mils DFT each / Manufacturer's Color Code : C901 (Aluminum) / Cure primer and top coats per manufacturer's specifications, then final cure at 400oF/205oC for 2 hours.",null,null,"Fill Out Gas Composition Tab"]
[null,"System E - 2 Coat Silicone Paint (Dry Temp. Resistance: 1000oF/538oC)\n(Surface Prep: Surface prep to near white metal SP-10 / Primer Coat: Carbozinc 11 Primer 3-4 mils DFT / Top Coat: Carboline Thermoline 4700, 2 coat at 1.5 mils DFT each / Manufacturer's Color Code : C901 (Aluminum) / Cure primer and top coats per manufacturer's specifications\nThe final cure for paint system E wil be at the customer site when it is exposed to the actual application temperatures.  Customer should expect/anticipate fumes to be present during initial exposure to elevated temperatures)",null,null,"Natural Gas "]
[null,"None "]
[null,"Special (Specify in Notes, Include Coating Spec and Paint System)"]
[]
["Wetted/Clamp-on"]
["Wetted "]
["Clamp-on"]

{"sheet":"Gas Composition Tab","index":2,"n_rows":38,"n_cols":13,"rows_kept":38,"cut":false,"hidden":false,"merged":[[0,10,0,12],[45,7,45,9],[46,7,46,9],[47,7,47,9],[48,7,48,9],[21,7,21,9],[22,7,22,9],[23,7,23,9],[24,7,24,9],[25,7,25,9],[26,7,26,9],[15,7,15,9],[16,7,16,9],[17,7,17,9],[18,7,18,9],[19,7,19,9],[0,2,0,4],[0,5,0,7],[43,7,43,9],[44,7,44,9],[33,7,33,9],[34,7,34,9],[35,7,35,9],[36,7,36,9],[37,7,37,9],[42,7,42,9],[27,7,27,9],[28,7,28,9],[29,7,29,9],[30,7,30,9],[31,7,31,9],[32,7,32,9],[20,7,20,9],[9,7,9,9],[10,7,10,9],[11,7,11,9],[12,7,12,9],[13,7,13,9],[14,7,14,9],[8,7,8,9],[2,7,2,9],[4,7,4,9],[5,7,5,9],[6,7,6,9],[7,7,7,9]]}
[null,null,"Case 1",null,null,"Case 2",null,null,null,null,"Case 3"]
["Gas name","  Mol wt","% Volume","fraction","mol Frac","% Volume","fraction","mol Frac",null,null,"% Volume","fraction","mol Frac"]
["Hydrogen (H2)",2.016]
["Nitrogen (N2)",28.013000000000002]
["Oxygen (O2)",31.99]
["Argon",39.948]
["Carbon Monoxide",28.01]
["Methane",16.042999999999999]
["Carbon Dioxide",44.011000000000003]
["Ethylene",28.053999999999998]
["Ethane",30.07]
["Hydr sulf (H2S)",34.076000000000001]
["Propylene",42.081000000000003]
["Propane",44.097000000000001]
["Isobutane",58.124000000000002]
["Normal butane",58.124000000000002]
["Butylene",56.107999999999997]
["Isopentane",72.150000000000006]
["Pentene",72.150000000000006]
["Pentane",72.12]
["Penatalyne",72.150000000000006]
["Hexane",101.19]
["Cyclohexane",86.17]
["Cyclopentane",70.13]
["Benzene",78.11]
["Heptane",100.203]
["Steam (water)",18]
["Mercaptan (NOM)",64.58]
["Ammonia",17.03]
["Helium(He2)",4]
["Fluorine(F2)",38]
["Uranium Hexafluoride(UF6)",352]
["Ethylene Oxide",44.05]
["Viny Chloride Monomer",62.5]
["Acetylene",26.04]
["Butadiene",54.09]
["Butene",56.11]
["Propadiene",40.06]