{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["опросный лист","Drop Downs"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"опросный лист","index":0,"n_rows":50,"n_cols":17,"rows_kept":50,"cut":false,"hidden":false,"merged":[[49,0,49,20],[46,12,46,14],[46,15,46,18],[46,19,46,20],[9,0,9,20],[20,0,20,20],[35,0,35,20],[40,4,40,11],[34,9,34,11],[34,12,34,15],[34,16,34,20],[31,4,31,8],[31,9,31,11],[31,12,31,15],[31,0,34,2],[45,12,45,20],[28,4,28,11],[28,12,28,20],[32,4,32,8],[17,4,17,9],[17,10,17,11],[40,12,40,15],[40,16,40,20],[37,4,37,11],[37,12,37,20],[29,12,29,20],[26,4,26,11],[4,0,4,11],[21,0,29,2],[5,0,8,2],[45,4,45,11],[41,4,41,11],[41,12,41,20],[43,12,43,15],[43,16,43,20],[42,4,42,7],[42,8,42,9],[42,10,42,11],[42,12,42,14],[42,15,42,18],[42,19,42,20],[43,10,43,11],[26,12,26,20],[31,16,31,20],[33,4,33,11],[32,9,32,11],[32,12,32,15],[14,17,14,19],[0,0,3,10],[0,13,3,20],[7,4,7,11],[8,9,8,11],[8,4,8,8],[5,4,5,11],[5,12,5,20],[6,4,6,11],[6,12,6,20],[7,12,7,20],[8,12,8,15],[8,16,8,20],[22,19,22,20],[15,13,15,16],[15,17,15,19],[16,13,16,16],[16,17,16,19],[19,4,19,8],[19,9,19,11],[19,12,19,15],[19,16,19,20],[18,4,18,8],[18,9,18,11],[18,12,18,15],[22,12,22,14],[22,15,22,18],[21,4,21,8],[21,10,21,11],[21,12,21,14],[48,4,48,11],[48,12,48,20],[30,0,30,20],[34,4,34,8],[44,10,44,11],[43,4,43,9],[44,4,44,9],[44,12,44,15],[44,16,44,20],[46,4,46,6],[46,7,46,9],[46,10,46,11],[47,12,47,20],[47,4,47,11],[33,12,33,20],[36,0,48,2],[39,12,39,15],[39,16,39,20],[39,4,39,8],[32,16,32,20],[36,4,36,8],[36,9,36,11],[36,12,36,15],[36,16,36,20],[10,0,19,2],[10,4,10,11],[10,12,10,20],[11,4,11,8],[11,9,11,11],[11,12,11,15],[11,16,11,20],[24,4,24,8],[24,9,24,11],[17,12,17,15],[17,16,17,20],[15,4,15,6],[15,7,15,9],[16,4,16,6],[16,7,16,9],[18,16,18,20],[14,4,14,8],[12,4,12,8],[13,4,13,8],[24,12,24,15],[24,16,24,20],[21,15,21,18],[21,19,21,20],[23,4,23,8],[12,13,12,16],[12,17,12,19],[13,13,13,16],[13,17,13,19],[14,13,14,16],[39,9,39,11],[38,4,38,8],[38,9,38,11],[38,12,38,15],[38,16,38,20],[25,4,25,8],[25,9,25,11],[25,12,25,15],[25,16,25,20],[29,4,29,11],[27,4,27,8],[27,9,27,11],[27,12,27,15],[27,16,27,20],[23,9,23,11],[23,12,23,15],[23,16,23,20],[22,4,22,8],[22,10,22,11]]}
[null,null,null,null,null,null,null,null,null,null,null,null,null,"GE Liquid Gas/Расходомер жидкости\nApplication Data Sheet/Опросный лист\nHighlighed Row = Mandatory Field\nВыделеные строки=Обязательны к заполнению"]
[]
[]
[]
["173021, Великий Новгород, ул. Нехинская 61                                                                                тел.: +7 (8162) 94-68-88      факс: +7 (8162) 94-67-75     E.mail:  office@dscontrols.ru"]
["GENERAL/Общие",null,null,1,"Company Name /Компания"]
[null,null,null,2,"Name/Контактное лицо"]
[null,null,null,3,"Address/Адрес"]
[null,null,null,4,"Phone/Тел.",null,null,null,null,"Email"]
[]
["PROCESS CONDITIONS/ Условия процесса",null,null,5,"Tag Number/\nНомер позиции"]
[null,null,null,6,"Fluid /Жидкость",null,null,null,null,"Stream Composition /\nСостав среды"]
[null,null,null,7,"Flow @ Standard Min.\nРасход@ Мин.",null,null,null,null,"Oper./\nНорм.","Max./\nМакс","Units/\nЕд."]
[null,null,null,8,"Temp. @ Flowrate Min. Температура @ Мин.",null,null,null,null,"Oper./\nНорм.","Max./\nМакс","Units/\nЕд."]
[null,null,null,9,"Press @ Flowrate Min./Давление @ Мин.",null,null,null,null,"Oper./\nНорм.","Max./\nМакс","Units/\nЕд."]
[null,null,null,10,"Visc @ Min/ \nВязкость Мин",null,null,"Oper. Viscosity/\nНорм",null,null,"Max./\nМакс","Units/\nЕд."]
[null,null,null,11,"Min Density /\nМин. Плотность",null,null,"Oper. Density/\nНорм. плотность",null,null,"Max./\nМакс","Units/\nЕд."]
[null,null,null,12,"Corrosive / Abrasive Property./\nАнтикоррозионая защита",null,null,null,null,null,"Build Up/\nОтложения"]
[null,null,null,13,"%Suspended Solids/\nТвердые включения %",null,null,null,null,"% Liquid Droplets/\nНаличие жидкости %"]
[null,null,null,14,"Design Max Press. /\nРасчетное давление",null,null,null,null,"Design Max.Temp./ \nРасчетная темп-ра"]
[]
["TRANSDUCER/\nFLOWCELL\nINSTALLATION/ Установка \nдатчика и измерительного участка",null,null,15,"Pipe Material/\nМатериал труб-да",null,null,null,null,"Pipe Size/\nРазмер \nтруб-да","Wall/Schd. /\nТолщина"]
[null,null,null,16,"Flange Rating/\nРейтинг фланца",null,null,null,null,"Lining/\nФутеровка","Pipe Spec/\nСтандарт \nтрубопровода"]
[null,null,null,17,"Upstream Straight Run\nНаличиие прямолинейного\nучастка до установки\nрасходомера",null,null,null,null,"Downstream /\nпосле установки\n расходомера",null,null,"(Pipe Diameters)/\n(Количество диаметров)",null,null,null,"(Pipe Diameters)/\n(Количество диаметров)"]
[null,null,null,18,"Pipe Orientation/\nОриентация \nтрубопровода",null,null,null,null,"Wetted / Clamp-On /\nВрезной/Накладной"]
[null,null,null,19,"Flowcell Required/\nТребуется измерительный \nучасток\n",null,null,null,null,"Isolation Valve (x'ducer)/\nОтсечной клапан\n (для датчика)"]
[null,null,null,20,"Transmitter Housing Requirement \nТребование к пылевлагозащите \nэлектронного блока"]
[null,null,null,21,"Transducer Haz. Area/\nТребование к \nвзрывозащите датчика",null,null,null,null,"Transmitter Haz Area /Требование к \nвзрывозащите\n электронного блока"]
[null,null,null,22,"Ambient Conditions (Corrosive gas, temp, hum)/\nУсловия окружающей среды (коррозионый газ, температура окружающего воздуха, влажность)\n"]
[null,null,null,23,"Required Cable Length (1000 ft. Max)/\nДлина кабеля (макс. 330 метров)"]
[]
["MEASUREMENT\nPARAMETERS/\nПараметры элетронного блока",null,null,24,"Analog Outputs\nАналоговые выходы",null,null,null,null,"Digital/Цифровой "]
[null,null,null,25,"Inputs (P and T)/\nВходы (P и Т)",null,null,null,null,"Alarms / Сигнальное реле"]
[null,null,null,26,"Power Available/ Напряжение питания"]
[null,null,null,27,"Desired Accuracy/\nТребование по\n погрешности",null,null,null,null,"Desired Repeatability/ \nТребования\n по повторяемости"]
[]
["FLOWCELL /Требования к измерительному участку ",null,null,28,"Flowcell Required \nНаличие измерительного участка",null,null,null,null,"Pipe Spec /Спецификация\n треубопровода"]
[null,null,null,29,"NDE Required (LPI, Hydro, X-ray are standard)/\nТребования по НК (Гидротест, Рентген, \nКапиллярная дефектоскопия- стандарт)"]
[null,null,null,30,"Material: Carbon Steel \nМатериал: Углеродистая сталь",null,null,null,null,"Stainless Steel \nНержавеющая сталь"]
[null,null,null,31,"5Cr-1/2Mo / \nХромомолибденовая \nсталь",null,null,null,null,"9Cr-1/2Mo\nХромомолибденовая \nсталь"]
[null,null,null,32,"Other Material :Specify Pipe and Flange /\nДругой материал: Укажите спецификацию \nтрубопровода и фланца",null,null,null,null,null,null,null,"Pipe: /Трубопровод",null,null,null,"Flange:/Фланец"]
[null,null,null,34,"Indicate Flowcell Flanged or Weld Prep Ends /\nУказать способ присоединение к трубопроводу- фланцевый или под приварку"]
[null,null,null,33,"Rating/Рейтинг",null,null,null,"Flange Type/\nТип фланца",null,"Pipe>24\"/\nТруба >24\""]
[null,null,null,35,"Addl Port Pressure - Size/Class\nТребование к присоединению датчика  давления - размер/класс",null,null,null,null,null,"Type /Тип"]
[null,null,null,36,"Addl Port Temp - Size/Class /\nТребование к присоединению датчика  температуры - размер/класс",null,null,null,null,null,"Type /Тип"]
[null,null,null,37,"Pipe Specification/ Спецификация трубопровода"]
[null,null,null,38,"Design P\nРасчетное давление",null,null,"Design Temp\nРасчетная \nТемпература",null,null,"Corro. Allow. \nПрипуск на коррозию"]
[null,null,null,39,"Paint Sytem /Требование по покраске"]
[null,null,null,40,"Interior Coating /Внутренне покрытие"]
["NOTES: Special Requirements (data logging, remote, totalization, calibration, etc.):\nSpecify any clearance issues (Submit Isometric if available): \nДополнение: Специальные требования (запись логов, удаленная настройка, наличие сумматора, калибровка)\nУкажите дополнительные требования (если имеется дополнительная изометрия трубопровода, просьба предоставить)"]

{"sheet":"Drop Downs","index":1,"n_rows":41,"n_cols":8,"rows_kept":41,"cut":false,"hidden":true,"merged":[]}
["Measurement location","Flowcell Required?","Transducer Removal ","Location","Transducer Haz Area","Transmitter Haz Area","Electronics Housing Requirement ","Transducer"]
["Horizontal Flow","Yes","Yes","Hazardous","General Purpose (Non-Haz)","None, NEMA4X & IP66","Weatherproof, Non-incendive NEMA4X & IP66 (Cl1 Div 2)","Clamp-On"]
["Vertical Flow (Up)","No (Hot/Cold Tap)","No","Nonhazardous","Weatherproo/NEMA4 / IP 65 ","USA/CAN Div2, Cl1 ABCD","Explosionproof NEMA7 / 4X","Wetted "]
["Vertical Flow (Down)",null,null,"Nonhazardous Weatherproof","Ex. Proof (CSA) Cl1 D1 Gr BCD","USA/CAN Div1, Cl1 BCD","Portable "]
["Other (Please Specify)",null,null,null,"Flameproof, II2 G Eex C T6 (ATEX)","ATEX II 2 G Ex d IIB+H2 T6","Intrinsically Safe "]
[null,null,null,null,"Flameproof SS, II2 G EEx d IIC T6 (ATEX)","ATEX II 2 G Ex d IIC T6","Other (List Requirments for Other)"]
[null,null,null,null,"Flameproof, II2 G Eex C T6 (IECEX)","IECEx Ex d IIB+H2 T6"]
[null,null,null,null,"Other (Specify in Notes)","IECEx Ex d IIC T6"]
[null,null,null,null,null,"INMETRO"]
[null,null,null,null,null,"Other (Specify in Notes)"]
[]
[]
[]
["Analog Outputs","Digital Outputs","Alarms","Inputs (Pres./Temp)","Power Available","NDE"]
["Two isolated 4 to 20","None","None","Isolated 4-20","100/120 VAC","X-Ray"]
["Six isolated 4 to 20","Four config. Pulse total/freq. outputs","Standard alarm relays","RDT","220/240 VAC","LPI"]
["Ten isolated 4 to 20","Modbus Digital","Hermetically sealed alarms ","Isolated 4-20 & RTD","12 to 28 VDC","HydroStatic"]
[null,"Modbus digital + 4 config. Pluse total/freq outputs",null,null,null,"Mag Particle "]
[null,"HART",null,null,null,"PMI"]
[null,"HART + 4 config. Pulse total/freq outputs",null,null,null,"Charpy Impact"]
[null,"MODBUS TCP",null,null,null,"Post Weld Heat Treatment"]
[null,"Ethernet card (panaview/OPC)",null,null,null,"NACE"]
[null,"Foundation Fieldbus",null,null,null,"Brinell Hardness"]
[null,"BACnet over Ethernet",null,null,null,"Others"]
[]
[]
["Carbon Steel ","Stainless Steel","5C-1/2M","9C-1/2M","Flange Rating","Flange Type","Flange Type","Flanged/Weld Prep"]
["ASTM A106 GrB/A105 (Valid to 24\" NPS)","ASTM A312 Gr304/A182 GrF304","ASTM A335 GrP5/A182 GrF5","ASTM A335 GrP9/A182 GrF9",150,"Weldneck","ANSI B16.47A","Flanged "]
["ASTM A672GrC70/A105 (Valid > 24\" NPS)","ASTM A312 Gr316/A182 GrF360","Other (Enter Below)","Other (Enter Below)",300,"Slip-on","ANSI B16.47B","Weld-Prep"]
["ASTM A333 Gr6/A350LF2","Other (Enter Below)",null,null,600,"RTJ",null,"Other"]
["Other (Enter Below)",null,null,null,900,"AWWA"]
[null,null,null,null,1500,"Other (Specify in Notes)"]
[null,null,null,null,2500]
["Port Type","Paint System ","Interior Coating ",null,"Other (Specify in Notes)"]
["Thredolet","System A - Bare Metal (Bare Steel, no coating)","Standard Water Soluable Rust Inhibitor "]
["Sockolet","System B -High Temperature Primer (Dry Temp. Resistance: 750oF/399oC)\n(Surface Prep: Surface prep to near white metal SP-10 / Primer Coat: Carbonic 11 Primer, 3-4 mils DFT, Manufacturer's Color Code 0700 (Gray) / Cure per Manufacturer's specifications)","Special (Specify in Notes, Include Coating spec and paint system)",null,"Gas Composition Tab"]
["Nipple","System C - 1 Coat Epoxy Paint, Self Priming (Dry Temp. Resistance: 425oF/218oC)\n(Surface Prep to near white metal SP-10 / Top Coat: Carboline Thermoline 450 Novalak Glass Filled Epoxy / Manufacturer's Color Code : 5742 (Gray), Cure per Manufacturer's specifications / Self Priming, No primer coat needed)","None",null,"Attaching Gas Composition to ADS"]
["Flanged","System D - 2 Coat Silicone Paint (Dry Temp. Resistance: 1000oF/538oC)\n(Surface Prep: Surface prep to near white metal SP-10 / Primer Coat: Carbozinc 11 Primer 3-4 mils DFT / Top Coat: Carboline Thermoline 4700, 2 coat at 1.5 mils DFT each / Manufacturer's Color Code : C901 (Aluminum) / Cure primer and top coats per manufacturer's specifications, then final cure at 400oF/205oC for 2 hours.",null,null,"Fill Out Gas Composition Tab"]
[null,"System E - 2 Coat Silicone Paint (Dry Temp. Resistance: 1000oF/538oC)\n(Surface Prep: Surface prep to near white metal SP-10 / Primer Coat: Carbozinc 11 Primer 3-4 mils DFT / Top Coat: Carboline Thermoline 4700, 2 coat at 1.5 mils DFT each / Manufacturer's Color Code : C901 (Aluminum) / Cure primer and top coats per manufacturer's specifications\nThe final cure for paint system E wil be at the customer site when it is exposed to the actual application temperatures.  Customer should expect/anticipate fumes to be present during initial exposure to elevated temperatures)"]
[null,"None "]
[null,"Special (Specify in Notes, Include Coating Spec and Paint System)"]